Spill Prevention, Control and Countermeasure Plan Checklist
No.	Assessment Items	Yes	No	N/A	Comments
1.	Is greater than 1,320 gallons of oil in above ground containers, or more than 42,000 gallons in underground storage tanks stored onsite?	☐	☐	☐
2.	Is the SPCC available onsite for each location where oil is stored?	☐	☐	☐
3.	Is the plan reviewed at least once every five years?	☐	☐	☐
4.	Is the plan amended within 6-months of any change which affects the Facility’s potential to discharge oil?	☐	☐	☐
5.	Are amendments implemented within 6-months of the date that the plan was changed?	☐	☐	☐
6.	Has management approved the plan?	☐	☐	☐
7.	Have resources been committed to implement the plan?	☐	☐	☐
8.	Does the plan include the following: Prediction of potential oil discharges from equipment and storage tanks including direction, rate of flow, and total quantity that may be discharged? Type of oil in each container and its storage capacity? Facility storm water drainage flow? Discharge/drainage controls (secondary containment, etc.)? Countermeasures for discharge discovery, response and cleanup? Emergency contact list and phone numbers? A facility diagram that describes the layout of the facility and the contents of each container, including buried tanks?	☐	☐	☐
9.	Are inspections and tests performed as described in the written procedures?	☐	☐	☐
10.	Are inspection records maintained onsite for three years?	☐	☐	☐
11.	Are all supplies available, as outlined in the plan?	☐	☐	☐
12.	Is secondary containment provided for oil filled equipment and bulk storage tanks?	☐	☐	☐
Spill Prevention, Control and Countermeasure Plan Checklist
No.	Assessment Items	Yes	No	N/A	Comments
13.	Have all applicable personnel trained in the operation and maintenance of equipment to prevent the discharge of oil?	☐	☐	☐
14.	Are personnel given spill prevention briefings at least annually?	☐	☐	☐
15.	Has a designated person accountable for oil spill prevention that reports to management?	☐	☐	☐
16.	Are spills cleaned up promptly?	☐	☐	☐
17.	Is oil stored in a secured area, including the following measures? Stored in a fully fenced area? Protected by locks and or guarded? Master flow and drain valves and pump controls are secured in the closed position when not in operation? Appropriate lighting is available?	☐	☐	☐

Revision Log
REVISION DATE	REVISION NO.	REVISION AUTHORITY	NATURE OF REVISION
12/03/2015	1	EH&S Coordinator	Date of Original Document Issuance

Controlled documents are maintained electronically.
Printed documents are UNCONTROLLED.
Prior to relying on a printed document, verify that it is current.